LA19-13-02 VNA
User Interface Software - V1.62 Installation

1. Uninstall any previous version of the software including VNAControl2.dll (select the 
   'Add/Remove Programs' from the Control Panel)

2. Run 'Setup' to install program

3. Calibration kit file (if provided) and other data files are in the 'data' subdirectory. Copy
   these to the subdirectory 'LA19-13-02' in your hard disk. For example, by using the
   command copy d:\data\*.* c:\LA19-13-02

Notes:

1. If you are using the DLL library, you may need to re-load the ActiveX reference from your client program 
   (e.g. in VEE, Automation References > VNA2 Control Library)

2. If you get a 'type mismatch' error when the program is first run, delete the file 'defcal.cal' in the
   c:\LA19-13-02 directory before running the program again.

3. If you need calibration kit data file(s) or an EEPROM data file please
   contact LA Techniques by sending your request to support@latechniques.com. 
   Please ensure you include the serial number of the calibration kit(s) and / or
   the serial number of the instrument.

4. This program only operates with the LA19-13-02 VNA. If you have the LA19-13-01 you need to a different 
   program (see the LA Techniques Ltd website)

5. If you are using an USB to RS232 adaptor, make sure that the COM port allocated is in the range 1 to 16.
   Refer to the Users Manual Getting Started section for further information.






